168 BORKA JOVANOVIĆ & UROŠEVIĆ

Fig. 9. The data retabulated to 0^∘.5 × 0^∘.5 resolution, for the following frequencies: 2720 MHz (top left), 1420 MHz (top right), 820 MHz (middle left), 408 MHz (middle right) and 34.5 MHz (bottom). The HPBWs for these frequencies are 0^∘.35, 0^∘.59, 1^∘.2, 0^∘.85 and 0^∘.7, respectively. The gray scales of temperatures are also given.