-0.7

-0.2

0.3

0.8

1.3

1.8

0.5 0.7 0.9 1.1 1.3 1.5

LOG (2xMEAN_AB18/arcsec)

LOG (RADIO/OPTICAL DIAMETER/arcsec)

PROCESSED FWHM

VIRTUAL PIXEL SCALE

EXTENDED 18 m FLAG LIMIT

EXTENDED 18 FLAG LIMIT

VIRTUAL PIXEL SCALE

PROCESSED FWHM

ONE-TO-ONE RELATION

0

0.2

0.4

0.6

0.8

1

1.2

-1 -0.5 0 0.5 1 1.5 2 2.5

LOG ( /arcsec)

NORMALISED SOURCE NUMBERS

LOGARITHMIC VARIATIONS IN THE DIAMETERS OF THE AKARI SOURCES

RADIO/OPTICAL DIAMETERS

AKARI 18 m DIAMETERS

FWHM OF THE AKARI PSF